RUMUAHIA EPC GAS GENERATOR CAT G3508 STARTER MOTOR EXHAUST OUTLET PIPING LAYOUT

3.6m

6.7m

0.6m

5.2m

1.3m

5.1m

Below is the quotation for materials to accomplish the CAT G3508 generator starter motor exhaust line installation.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S/N | Description | Quantity | Cost | Total Cost |
| 1 | 2”” Galvanize pipes | 4 | 4700 | N18800 |
| 2 | 2” Galvanize Elbow | 8 | 1200 | N9600 |
| 3 | 2” Galvanize Socket | 2 | 1200 | N2400 |
| 4 | Thread Tape | 5 | 100 | N500 |
| 5 | Threading | 16 | 500 | N8000 |
| 6 | Transport | 1 | 5000 | N5000 |
|  | Total |  |  | N51300 |